**plumbing question 2- cleanouts**

question 1:

how big interval shall between two cleanouts on a 4” horizontal sanitary drainage pipe?

section 7.4.7.2 Size and Spacing of Cleanouts (1) (b)

answer: 15m

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

question 2:

how big interval shall between two cleanouts on a 6” horizontal sanitary drainage pipe?

section 7.4.7.2 Size and Spacing of Cleanouts (1) (c)

answer: 30m

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

question 3:

how many cleanouts shall be placed on a 6” horizontal sanitary drainage pipe with two 90-degree direction changes?

section 7.4.7.1 （5）Cleanouts for Drainage Systems. & section 7.4.7.2 Size and Spacing of Cleanouts (1) (c)

answer: every 30m and at each 90-degree direction change.